
\section{Cable Labels}

The next page contains cable labels for one supermodule. Two rows of
labels are needed to mark one set of cables. The upper two sets are
for anode and drift high-voltage, then there are three sets to mark
both ends of the DCS power cables and the RJ-45 end of the ethernet
cables.

\newpage

\setlength{\TPHorizModule}{12.55mm}
\setlength{\TPVertModule}{28.70mm}
\textblockorigin{0mm}{14.5mm}


\newcommand{\clabel}[3]{
\begin{textblock}{1}(#1,#2)
\center \textsf{#3}
\end{textblock}
}

\thispagestyle{empty}


%\newcommand{\clabels}[2]{
%\multido{\ny=#1+1,\nlstart=0+3}{2}{ %
%  \multido{\nl=\nlstart+1,\nxstart=0+5}{3}{ %
%    \multido{\nx=\nxstart+1,\ns=0+1}{5}{ %
%      \clabel{\nx}{\ny}{} %
%}}}
%}



% Anode HV labels

\multido{\ny=0+1,\nlstart=0+3}{2}{ %
  \multido{\nl=\nlstart+1,\nxstart=0+5}{3}{ %
    \multido{\nx=\nxstart+1,\ns=0+1}{5}{ %
      \clabel{\nx}{\ny}{A$^{L}$\nl{}$^{S}$\ns{}} %
}}}

% Drift HV labels

\multido{\ny=2+1,\nlstart=0+3}{2}{ %
  \multido{\nl=\nlstart+1,\nxstart=0+5}{3}{ %
    \multido{\nx=\nxstart+1,\ns=0+1}{5}{ %
      \clabel{\nx}{\ny}{D$^{L}$\nl{}$^{S}$\ns{}} %
}}}

% Other labels (LxSy)

\multido{\nystart=4+2}{3}{ %
\multido{\ny=\nystart+1,\nlstart=0+3}{2}{ %
  \multido{\nl=\nlstart+1,\nxstart=0+5}{3}{ %
      \multido{\nx=\nxstart+1,\ns=0+1}{5}{ %
          \clabel{\nx}{\ny}{L\nl{}S\ns{}} %
}}}}




