\section{How to start the low voltage FSM}

The low voltage FSM runs on two different computers. The first one is the LV01 and the second
one PVSS03 where the user interface is running. 

Normally there is no necessarity to log in into LV01 except in case of a power failure on LV01
or a program crash. In this cases you have to log in and perform the following steps:

\begin{compactenum}
\item Start PVSS
\item Start project \select{trd\_lv} and open the log viewer
\item Wait until \msg{update} appears in log viewer
\item Start \select{pvss\_dim\_manager} (should be last one in list)
\item Open \select{DeviceEditorNavigator}; in \select{FSM view} click on \select{navigator
  mode} and then click on button \select{start / restart all}
\end{compactenum}

\vspace{\baselineskip}
On PVSS03 you have to take the following steps:
\begin{compactenum}
\item Start PVSS
\item Start project \select{trd\_fee}
\item Start \select{trd\_ConfigureFeeCom}
\item Start \select{PVSS00dim3.6}
\item Open \select{DeviceEditorNavigator}; in \select{FSM view} click on \select{navigator
  mode} and then click on button \select{start / restart all}
\item Start \select{dcsUi/dcs} and log in with your username / password
\end{compactenum}

\vspace{\baselineskip}
In case of a restart of PCU you have to do following in the PVSS project on PVSS03:
\begin{compactenum}
\item Set \select{pcu\_channel} to on
\item Set \select{dcs\_pdf channel} to on
\item In \select{pcuControl} set timeout to 10
\end{compactenum}

\vspace{\baselineskip}
\emph{Remark:} If PVSS has chrashed on PVSS03 you also have to kill the programm
\select{smiSM.exe} via the windows taks manager
