
\section{Preparation of Supermodule Hull}


\subsection{DCS Power Distribution}

The lengths of the DCS power cables for one supermodule are given in
this table:

\begin{tabular}{|l|rrrrr|}
\hline
          & Stack 0 & Stack 1 & Stack 2 & Stack 3 & Stack 4 \\
\hline
Layer 3-5 &  800 cm &  650 cm &  500 cm &  390 cm &  240 cm \\
Layer 0-2 &  700 cm &  570 cm &  440 cm &  335 cm &  215 cm \\
\hline
\end{tabular}

%The cables should be labelled on both sides 


\subsection{Checklist}

\begin{itemize}
\checkitem {end frames correctly oriented}
\checkitem {sheets mounted on frames between S1/S2 and S2/S3}
\checkitem {all screws well sunk}
\checkitem {screws inserted in bottom corner ledges for stepframes 
  (S0/S1, S3/S4)}
\checkitem {holes in side-walls covered with tape from inside}
\checkitem {power bus bar connections checked}
\checkitem {cables securely fixed in LV endcap patch panel}
\checkitem {HV patch boxed prepared with cable ties and fixation screws}
\checkitem {PDB + cables installed}
\checkitem {Sch\"utten box installed}
\end{itemize}

