\chapter{Super-Module Integration}

\section{Hull}

\begin{figure} [bht]
\begin{center}
\includegraphics[width=\textwidth]{figs/dietel/pbb.pdf}
\caption{\label{fig:hull:pbb} Cabling of Power Bus Bars. Blue numbers
  show places for ORI power cables, blue dots indicate holes left
  empty. All ROB cables except for the one in the middle should be
  mounted. Note the orientation of the cables. }
\end{center}
\end{figure}


\begin{figure} [bht]
\begin{center}
\includegraphics[width=\textwidth]{figs/dietel/sidewall_a.pdf}
\caption{\label{fig:hull:sidewall_a} Assemly of sidewall on side A,
  i.e. the right side when looking into the magnet if the SM is
  installed in sector 4.  The cooling profiles LxR should be
  used. This drawing does not apply to super-modules in sectors
  12--15, which will be supplied from the A-side.}
\end{center}
\end{figure}

\begin{figure} [bht]
\begin{center}
\includegraphics[width=\textwidth]{figs/dietel/sidewall_b.pdf}
\caption{\label{fig:hull:sidewall_b} Assemly of sidewall on side B,
  i.e. the left side when looking into the magnet if the SM is
  installed in sector 4.  The cooling profiles LxL should be
  used. This drawing does not apply to super-modules
  in sectors 12--15, which will be supplied from the A-side.}
\end{center}
\end{figure}




\section{SMEC Patchpanel}


\begin{figure} [bht]
\begin{center}
\includegraphics[width=0.90\textheight, angle=90]{figs/oyama/20070412-SMECPP.pdf}
\caption{\label{fig:SMECPP-design}
Design of Patch Panel on Super-module End-Cap.
}
\end{center}
\end{figure}
