\chapter{Frontend Readout Rates with New Data Formats}

\section{Preliminary Material}

\begin{table}[h]
  \begin{center}
    \begin{tabular}{llll}
        & ZS ADC Data & Reduced Raw Data & Tracklet Data\\ \hline \hline
      FEE event readout time [us/event] & 36.5 & 19.5 & 7\\
      FEE readout rate at 100\% deadtime [ kHz ] & 27.4 & 51.2 & \<143 (100)\\
      Readout data throughput at maximal FEE readout rate [ GB/s ] & 81.5 & 33.4 & \<38.2 (26.7)\\
      Readout rate at 50 kHz interaction rate [ kHz ] & 17.7 & 25.3 & 37\\
      Corresponding readout data throughput [ GB/s ] & 52.4 & 16.5 & 9.7\\
      Corresponding deadtime [ \% ] & 65 & 49 & 26\\
      In () numbers for 100kHz max. rate\\
      \hline
    \end{tabular}
  \end{center}
  \caption{Readout rates for different TRD data formats}
\end{table}
